<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="50.83" x2="0" y2="2.5" width="0" layer="20"/>
<wire x1="0" y1="2.5" x2="2.5" y2="0" width="0" layer="20"/>
<wire x1="2.5" y1="0" x2="57.368" y2="-0.254" width="0" layer="20"/>
<wire x1="57.368" y1="-0.254" x2="57.321953125" y2="2.404778125" width="0" layer="20"/>
<wire x1="57.321953125" y1="2.404778125" x2="59.912146875" y2="5.0109375" width="0" layer="20"/>
<wire x1="59.912146875" y1="5.0109375" x2="59.809484375" y2="37.7148375" width="0" layer="20"/>
<wire x1="59.809484375" y1="37.7148375" x2="57.283425" y2="40.4506" width="0" layer="20"/>
<wire x1="57.283425" y1="40.4506" x2="57.12" y2="51.74" width="0" layer="20"/>
<wire x1="57.12" y1="51.74" x2="55.59" y2="53.33" width="0" layer="20"/>
<wire x1="55.59" y1="53.33" x2="2.5" y2="53.33" width="0" layer="20"/>
<wire x1="2.5" y1="53.33" x2="0" y2="50.83" width="0" layer="20"/>
<text>F1 Power Control</text>
<text>F2 Power Control</text>
<text>Stir Shield</text>
<text>https://github.com/micworg/stir</text>
</plain>
<libraries>
<library name="stir_shield">
<packages>
<package name="4PIN">
</package>
<package name="1PIN">
</package>
<package name="2PIN">
</package>
<package name="BUTTON">
</package>
<package name="5PIN_KY-04">
</package>
<package name="5PIN_LCD">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0805-THM">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD_NOLABELS">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections, no silk labels. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FAN1" library="stir_shield" package="4PIN" value="4PIN">
<attribute name="NAME"/>
</element>
<element name="FAN1-POW-CON" library="stir_shield" package="1PIN" value="1PIN"/>
<element name="FAN2" library="stir_shield" package="4PIN" value="4PIN">
<attribute name="NAME"/>
</element>
<element name="FAN2_POW_CON" library="stir_shield" package="1PIN" value="1PIN"/>
<element name="R1" library="adafruit" package="0805-THM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0805-THM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0805-THM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0805-THM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="stir_shield" package="2PIN" value="2PIN"/>
<element name="KY-040" library="stir_shield" package="5PIN_KY-04" value="5PIN_KY-04">
<attribute name="NAME"/>
</element>
<element name="LCD" library="stir_shield" package="5PIN_LCD" value="5PIN_LCD">
<attribute name="NAME"/>
</element>
<element name="B1" library="SparkFun-Boards" package="UNO_R3_SHIELD_NOLABELS" value="ARDUINO_UNO_R3_SHIELDNOLABELS"/>
<element name="RESET" library="stir_shield" package="BUTTON" value="BUTTON">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="FAN1" pad="P$2"/>
<contactref element="FAN2" pad="P$2"/>
<contactref element="B1" pad="VIN"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="FAN1" pad="P$4"/>
<contactref element="B1" pad="D9"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="FAN2" pad="P$4"/>
<contactref element="B1" pad="D10"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="KY-040" pad="P$2"/>
<contactref element="LCD" pad="P$2"/>
<contactref element="B1" pad="5V"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="FAN1" pad="P$3"/>
<contactref element="B1" pad="D2"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="FAN2" pad="P$3"/>
<contactref element="B1" pad="D3"/>
</signal>
<signal name="N$9">
<contactref element="FAN2_POW_CON" pad="P$1"/>
<contactref element="B1" pad="D7"/>
</signal>
<signal name="RESET">
<contactref element="B1" pad="RES"/>
<contactref element="RESET" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="KY-040" pad="P$1"/>
<contactref element="B1" pad="GND@0"/>
<contactref element="FAN1" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="FAN2" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="LCD" pad="P$1"/>
<contactref element="RESET" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="B1" pad="D8"/>
<contactref element="FAN1-POW-CON" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="LCD" pad="P$5"/>
<contactref element="B1" pad="D11"/>
</signal>
<signal name="N$10">
<contactref element="LCD" pad="P$4"/>
<contactref element="B1" pad="SCL"/>
</signal>
<signal name="N$11">
<contactref element="LCD" pad="P$3"/>
<contactref element="B1" pad="SDA"/>
</signal>
<signal name="N$12">
<contactref element="KY-040" pad="P$3"/>
<contactref element="B1" pad="D4"/>
</signal>
<signal name="N$13">
<contactref element="KY-040" pad="P$4"/>
<contactref element="B1" pad="D6"/>
</signal>
<signal name="N$14">
<contactref element="KY-040" pad="P$5"/>
<contactref element="B1" pad="D5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
